***VANTAGE – METRO SERIES THERMAL HEART***

**5.8 SLIDING DOORS**

*Metro Series ThermalHEART sliding doors are rated to 2.7m high in ‘extra high’ wind zones. They slide on an external track with a fixed sidelight. Stiffening boxes on interlocker stiles and mullions align in the closed position.*

Doors shall be constructed using the Metro Series ThermalHEART sliding door frame and an IGU thickness up to 44mm.

* Opening sashes are possible if placed away from the travel path of an opening door panel.
* Sidelights and overlights are possible through the use of either an integral mullion/transom or by using a coupling bar with the Metro ThermalHEART awning window frame.

Applies to Door No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*