**Specification for Residential Series ThermalHEART Windows & Doors**

9 February 2023

***ALTHERM RESIDENTIAL SERIES THERMALHEART RANGE***

**3.2 HORIZONTAL SLIDING WINDOWS**

Windows shall be constructed using Residential Series ThermalHEART sliding window frames and an IGU thickness up to 24mm.

* The perimeter frame is the Residential Series ThermalHEART sliding door frame with narrower profile for window rails *(22340)*. The small interlocker mullion is also generally used.
* Interlocker stiles and mullions are flush in the closed position.
* An overlight transom *(22500)* allows overlights to be in used in association with sliding panels.
* All fixed lights and moving panels are externally beaded.

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*