**Specification for APL Architectural Series Windows & Doors**

1 July 2013

***ALTHERM – APL ARCHITECTURAL SERIES***

**6.6 HINGED and FRENCH DOORS**

*APL Architectural Series hinged and French doors are rated to 2.7m high in ‘very high’ wind zones.*

*For French doors rebated meeting stiles give a flush appearance and provide superior weathering. Parliament hinges allow doors to open a full 180° in a brick veneer application.*

Doors shall be constructed using APL Architectural Series hinged door frames, utilising panels with an IGU thickness up to 26mm.

* Standard configuration

Open In / Open Out

Applies to Door No’s... *(or refer to the window schedule drawing)*

* Hardware as nominated in the hardware section.
* Options = ...

*(options = parliament hinges, bottom rail extender)*

Applies to Door No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*