**Specification for Metro Series Windows & Doors**

1 July 2013

***ALTHERM - METRO SERIES***

**4.1 AWNING and CASEMENT WINDOWS**

Windows shall be constructed using Metro Series frames, utilising a 40mm platform and an IGU thickness up to 26mm.

* Opening sashes include a non-facing sash as standard though a cover facing option is available.
* All windows are externally beaded with square edge rather than sloped beads.

*( for single glazing there is an option to use sloping beads)*

* Mullions and transoms have internal or external stiffening fins or boxes depending on window span and customer preference.

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*