**Specification for Residential Series ThermalHEART Windows & Doors**

9 February 2023

***ALTHERM RESIDENTIAL SERIES THERMALHEART RANGE***

**3.8 SLIDING DOORS**

*Residential Series ThermalHEART sliding doors are rated to 2.2m high in ‘extra high’ wind zones. They slide on an internal track with fixed or sashed sidelight. Stiffening boxes (where required) on interlocker stiles, meeting stiles, and mullions are available.*

Doors shall be constructed using the Residential Series ThermalHEART sliding door frame and an IGU thickness up to 24mm.

* Opening sashes are possible in the adjoining fixed panel.
* Overlights are possible through the use of an overlight transom at the head of the sliding door frame.

Applies to Door No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*