***FIRST - APL ARCHITECTURAL SERIES THERMAL HEART*®**

**5.2 HORIZONTAL SLIDING WINDOWS**

Windows shall be constructed APL Architectural Series ThermalHEART**®** sliding window frames and an IGU thickness up to 44mm.

* The perimeter frame is the APL Architectural Series ThermalHEART**®** sliding door frame with smaller profiles for rails, stiles and mullions.
* Stiffening boxes on interlocker stiles and mullions align in the closed position.
* All windows are externally beaded with square edge rather than sloped beads.

Applies to Window No’s... *(or refer to the window schedule drawing)*

*For alternative options contact APL Technical Support*